-5187 FFFFEBBD NCERR BAD IPX CONFIG

Source

NCP™ Engine

Explanation

The NCP Engine found incorrect configurations of multiple IPX/SPX addresses.

Possible Solution

With multiple network adapters, you must set a non-zero internal network number for the IPX addresses.

Action

See Reporting Error Code Problems to Novell®.

A trademark symbol (®, TM, etc.) denotes a Novell trademark. An asterisk (*) denotes a third-party trademark. For information on trademarks, see Legal Notices.