-636 FFFFFD84 UNREACHABLE SERVER

Source

eDirectory™

Explanation

An attempt to perform a partition operation failed. The partition operation was flagged to ensure all of the eDirectory servers within the replica ring of the partition root object were available.

Possible Cause

One of the eDirectory servers in the replica ring was unavailable due to a transport failure, error -625.

Action

Resolve the communication error between the server responding to the client's request for a partition operation and the server in the replica ring that is unavailable.

Examine the Replica Synchronization status on the server holding the master replica and resolve any -625 (ERR_TRANSPORT_FAILURE) errors.

To ensure that each server in the replica ring is available, the following partition operations can be flagged when submitting the request:

- Add Replica
- Remove Replica
- Split Partition
- Merge Partition
- Change Replica Type
- Repair Timestamps

A trademark symbol (®, TM, etc.) denotes a Novell trademark. An asterisk (*) denotes a third-party trademark. For information on trademarks, see Legal Notices.