-119 FFFFFF89 BUFFER TOO SMALL

Source

eDirectory™ operating system

Explanation

The data to be passed back is too large for the buffer that was declared.

Warning:

Applying all solutions mentioned in this topic could make the problem worse if the actual cause of the problem is not known. Before following a course of action, make sure that you understand the cause of the error and the consequences for the actions suggested.

Possible Cause

An occurrence of this error can indicate that the eDirectory server has insufficient IPX* sockets available.

Action

Increase the maximum number of open IPX sockets allowed by the operating system.

Possible Cause

An internal eDirectory error occurred.

Action

Contact a Novell support provider.

Possible Cause

If this error occurs in response to an attempt to bind multiple LAN cards, the cause could be that the license does not allow it or it is not installed.

Action

Make sure the license to the server is installed and allows the number of connections desired.

Possible Cause

This error can occur when you are attempting to bind multiple LAN cards and the product being used is the NetWare Connect product that ships with intraNetWare for Small Business (IWSB). In this case, the problem will prevent binding IPX to a physical LAN card and NetWare Connect's PPPRNS service.

Action

If the product being used has one of the following serial numbers, get and apply the patch IWSBP1.exe that is available from Novell technical support on the Web at http://support.novell.com/search/ff_index.htm.

The serial numbers are in the following ranges:

- 20624444 to 20624657
- 61717237 to 62244253
- 79005005 to 79010004.

A trademark symbol (®, TM, etc.) denotes a Novell trademark. An asterisk (*) denotes a third-party trademark. For information on trademarks, see Legal Notices.