-680 FFFFFD58 TRANSPORT MODIFIED

Source

eDirectory™

Explanation

An inconsistency occurred when attempting to connect to the target server.

Warning:

Applying all solutions mentioned in this topic could make the problem worse if the actual cause of the problem is not known. Before following a course of action, make sure that you understand the cause of the error and the consequences for the actions suggested.

Possible Cause

An attempt to establish a connection with the target server returned a Transport Failure error (-625). However, an auxiliary attempt succeeded by renegotiating the NetWare* Core Protocol* (NCP) connection's IPX Maximum Packet Size, IPX* Packet Signature, or IPX Packet Checksumming.

Action

Make sure the transport components are working.

Possible Cause

Faulty LAN drivers, LAN cards, or other LAN/WAN equipment might exist between the source and target servers.

Action

Make sure that any LAN/WAN equipment, cards, and drivers that exist between the source and target server are functioning properly.

A trademark symbol (®, TM, etc.) denotes a Novell trademark. An asterisk (*) denotes a third-party trademark. For information on trademarks, see Legal Notices.