-5896 FFFFE8F8 SERR SKTEFAULT

Source

SAL*

Explanation

Bad address detected in socket operation.

Possible Cause

The system detected an invalid pointer address in attempting to use a pointer argument of a call. This error occurs if an application passes an invalid pointer value, or if the length of the buffer is too small. For example, if the length of an argument, which is a SAL_SOCKADDR structure, is smaller than the size of (SAL_SOCKADDR).

Action

Contact a Novell® support provider.

A trademark symbol (®, TM, etc.) denotes a Novell trademark. An asterisk (*) denotes a third-party trademark. For information on trademarks, see Legal Notices.