Web Chaining

| ISA Server supports routing requests from clients to an upstream ISA Server computer or to an alternate location. For Web Proxy client requests, create Web chaining rules to specify how such requests are routed. Note For Firewall client and SecureNAT client requests, use firewall chaining to specify how requests will be routed.
| How To... You can perform the following tasks:
| Create a Web chaining rule: On the Tasks tab, click Create New Web Chaining Rule.
| Define SSL bridging for a rule: In the details pane, select a rule, and then on the Tasks tab, click Define SSL Bridging for Selected Rule.
| Modify a rule: In the details pane, select a rule, and then on the Tasks tab, click Edit Selected Rule.
| Delete rules: In the details pane, select one or more rules, and then on the Tasks tab, click Delete Selected Rules.
| Disable rules: In the details pane, select one or more rules, and then on the Tasks tab, click Disable Selected Rules.
| Configure firewall chaining: On the Tasks tab, in Related Tasks, click Define Firewall Chaining Properties.
| Configure dial-up properties: On the Tasks tab, in Related Tasks, click Specify Dial-up Preferences.
| Related Topics For more information, see these topics in ISA Server Help:
| Multi-Networking: Concepts
| Web chaining rules
| Firewall chaining
| ISA Server Online